

**RISK ASSESSMENT FINDINGS**

|  |  |
| --- | --- |
| **Department/Service** |  |
| **Date** |  |
| **Assessor** |  |
| **Approved By** |  |
| **Review Date** |  |

**Relevant Legislation:**

The Management of Health and Safety at Work Regulations 1999

**RISK ASSESSMENT RECORD**

**ACTIVITY and/or ENVIRONMENT TO BE ASSESSED: Plastering - Vocational training**

**DATE:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **KEY (People at risk)** | **Likelihood (L)** | **Severity (S)** | **Risk Calculation** | **Risk Rating** |
| E = Employee YP = Young PersonsP = Public C = ContractorsV = VisitorsEM = Expectant Mothers | 1. Very Low (rare/very unlikely)2. Low (unlikely)3. Medium (could occur/possible)4. High (likely to occur/probable)5. Very High (near certain to occur)  | 1. Insignificant (nuisance/discomfort)2. Minor (no lost time)3. Moderate (time loss)4. Significant (serious/incapacity to work)5. Major (Death) |  Likelihood x Severity=Rating | **1- 6** **LOW RISK** Monitor * 1. **MEDIUM RISK** Monitor, review & reduce risk where possible

**14-25** **HIGH RISK** Further Action Required |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **1.Hazards Identified and potential harm it could cause** | **2. People****At Risk** | **3.Controls in Place** | **4.Risk Rating** | **5. Further Action Required/ Recommendations** | **6.Target Date for Completion** |
| **L** | **S** | **Score** | **Risk** |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Working at height |  | Refer to working at height risk assessment |  |  |  |  |  |  |
| Manual handling |  | Refer to manual handling risk assessment |  |  |  |  |  |  |
| Hazardous substances |  | Refer to COSHH risk assessments for individual hazardous substances |  |  |  |  |  |  |
| Slips and trips |  | Refer to preventing slips and trips risk assessment |  |  |  |  |  |  |
| Accident / incident |  | Ensure adequate first aid arrangements are in place including qualified first aid at work staff. |  |  |  |  |  |  |
| Fire |  | Refer to fire safety risk assessment |  |  |  |  |  |  |
| Dry plaster mix |  | * Pupils briefed on the risks of dry plaster powder and know to avoid skin contact, excessive dust build-up and contact with eyes.
* Work area suitable to prevent excessive dust build-up.
* Water supply nearby to wash dust off skin.
* Pupils to wear eye protection when plastering.
* Gloves and barrier creams available.
 |  |  |  |  | Adequate supervision of pupils |  |
| Electricity |  | * Supervisor to turn of power while plastering work ongoing if required.
* Use of 110 v supply and RCDs where necessary.
* Regular documented checks of equipment and PAT testing.
* Procedure in place for defective equipment.
 |  |  |  |  | Adequate supervision of pupils |  |
| Hygiene |  | Adequate washing facilities on site. |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |